**TEAM 2**

**Name**: Mike Nitchie and Bharat Kumar Kuncharavelu

REVIEW:

* Given a baud rate and BRGH set or clear, be able to determine the value that must be placed into SPBRG register to get the given baud rate.
* Know the difference between Asynchronous and Synchronous communications.
* What registers are involved in USART transmission and reception. What registers are they in.
* Know which pins the USART uses for serial communications.
* Know how to enable Asynchronous communication and enable PORTB pins 1 and 2 to be serial port pins. ( configureModes sub routine in code).